[system]
systemname = OBP60v
loglevel = 3
deviceid = 100
simulation = on
histpath = ~/.local/lib/obp60v
guistyle = default
mouseptr = on

[gui]
win_x = -1
win_y = -1

[can]
enabled = false
interface = can0

[nmea0183]
enabled = false
port = /dev/ttyV1

[network]
enabled = false
address = 127.0.0.1
port = 10110

[bme280]
enabled = false
port = 1
address = 0x76

[gps]
enabled = false
port = /dev/ttyACM0

[opencpn]
navobj = ~/.opencpn/navobj.xml
config = ~/.opencpn/opencpn.conf

[tracker]
type = NONE
host = 127.0.0.1
port = 80
path = /
ssl = false
username = demo
password = secret
mqtt_host = 127.0.0.1
mqtt_port = 1883
mqtt_ssl = false
mqtt_user = demo
mqtt_pass = 123456
trace = false

[boat]
name = My boat
sailno = GER 815
class = One off
handicap = 100.0
club = NONE
team = OBP

[settings]
timezone = 1
boat_draft = 1.3
fuel_tank = 17
fuel_consumption = 1.5
water_tank_1 = 47
water_tank_2 = 50
battery_voltage = 12
battery_type = AGM
battery_capacity = 200
solar_power = 0
generator_power = 0

[units]
length_format = m
distance_format = nm
speed_format = kn
wind_speed_format = ln
temperature_format = C
date_format = ISO

[display]
hold_values = off
backlight_color = red
flash_led_mode = limit

[buzzer]
buzzer_gps_error = off
buzzer_gps_fix = off
buzzer_by_limits = off
buzzer_mode = off
buzzer_power = 50

[pages]
number_of_pages = 10
start_page = 1

[page1]
type = Clock

[page2]
type = Barograph

[page3]
type = Anchor

[page4]
type = XTETrack

[page5]
type = Wind

[page6]
type = TwoValues
value1 = LAT
value2 = LON

[page7]
type = ThreeValues
value1 = COG
value2 = STW
value3 = DBT

[page8]
type = FourValues
value1 = AWA
value2 = AWS
value3 = COG
value4 = STW

[page9]
type = Rudder

[page10]
type = SkyView
